IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "Projektnummer"
Time stamp: "2019-09-02T08:40:27"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20160225_1515(x64) - Exporter 17.0.416.0 - Alternate UI 17.12.14.0"
Application: "Autodesk Revit 2017 (ENU)" version "2017" identifier "Revit" by Organization "Autodesk Revit 2017 (ENU)"

People and organizations
  Person "Peace" of Organization (no name given)
  Owner history of Person "Peace" of Organization (no name given) | application "Autodesk Revit 2017 (ENU)" version "2017" identifier "Revit" by Organization "Autodesk Revit 2017 (ENU)" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "Projektnummer" | long name "Projektname" | phase "Projektstatus"
  IFCSITE "Default" | latitude 42° 12′ 46.804504″ | longitude -71° 2′ 0.602416″ | elevation above sea level 0.
    IFCBUILDING | postal address: "## Straße Ort, Bundesland PLZ", "Boston", "MA"
      IFCBUILDINGSTOREY "Ebene 1" | long name "Ebene 1" | elevation 0.
        contains 1 element
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "LOROWERK 01005-125X" | object type "LOROWERK 01005-125X" | names: "LOROWERK 01005-125X:LOROWERK 01005-125X:229838" | material: materials ("ConnectorOutletMediumMaterial", "ConnectorInletMediumMaterial", "Material_3012") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Constraints, Dimensions, Graphics, Insulation

Types
  IFCPIPEFITTINGTYPE "LOROWERK 01005-125X" | 1 occurrence | material: materials ("ConnectorOutletMediumMaterial", "ConnectorInletMediumMaterial", "Material_3012") | property sets: Data, Dimensions, General, Identity Data, Other

Property sets
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
    Client Name = "Besitzer" (IFCTEXT)
    Project Address = "## Straße Ort, Bundesland PLZ" (IFCTEXT)
    Project Issue Date = "Ausgabedatum" (IFCTEXT)
    Project Name = "Projektname" (IFCTEXT)
    Project Number = "Projektnummer" (IFCTEXT)
    Project Status = "Projektstatus" (IFCTEXT)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Other | properties | on 1 object (1 IFCFLOWFITTING)
    Category = "Pipe Fittings" (IFCLABEL)
    Family = "LOROWERK 01005-125X: LOROWERK 01005-125X" (IFCLABEL)
    Family and Type = "LOROWERK 01005-125X: LOROWERK 01005-125X" (IFCLABEL)
    Type = "LOROWERK 01005-125X: LOROWERK 01005-125X" (IFCLABEL)
    Type Id = "LOROWERK 01005-125X: LOROWERK 01005-125X" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: 8 mm Kopf" (IFCLABEL)
    Family and Type = "Level: 8 mm Kopf" (IFCLABEL)
    Type = "Level: 8 mm Kopf" (IFCLABEL)
    Type Id = "Level: 8 mm Kopf" (IFCLABEL)
  Other | properties | on 1 type object
    Category = "Pipe Fittings" (IFCLABEL)
    Family Name = "LOROWERK 01005-125X" (IFCTEXT)
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "8 mm Kopf" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Ebene 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    DATANORM = "01005.125X" (IFCTEXT)
    Description = "LORO-X Stahlabflussrohre" (IFCTEXT)
    GTIN = "4038088005118" (IFCTEXT)
    HAN = "01005.125X" (IFCTEXT)
    Manufacturer = "LOROWERK K.H. Vahlbrauk GmbH & Co. KG" (IFCTEXT)
    OmniClass Number = "" (IFCTEXT)
    OmniClass Title = "" (IFCTEXT)
    Type Name = "LORO-X Rohre mit einer Muffe" (IFCTEXT)
    VDIBSN = "020001???001001???00100100000100300700000000000001000000040000800000" (IFCTEXT)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCFLOWFITTING)
    Manufacturer = "LOROWERK K.H. Vahlbrauk GmbH & Co. KG" (IFCLABEL)
  Pset_DistributionFlowElementCommon | properties | on 1 object (1 IFCFLOWFITTING)
    Reference = "LOROWERK 01005-125X" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCFLOWFITTING)
    Host = "Level : Ebene 1" (IFCTEXT)
    Level = "Level: Ebene 1" (IFCLABEL)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Dimensions | properties | on 1 object (1 IFCFLOWFITTING)
    Area = 0.937860337575891 (IFCAREAMEASURE) [SQUARE_METRE]
    Maximum Size = 125. (IFCLENGTHMEASURE) [MILLI METRE]
    Minimum Size = 125. (IFCLENGTHMEASURE) [MILLI METRE]
    Size = "125 mmø-125 mmø" (IFCTEXT)
    Volume = 0.0672322022142209 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 type object
    CONNECTOR0_DIAMETER_dZ_0r = 125. (IFCLENGTHMEASURE) [MILLI METRE]
    CONNECTOR0_dZ_00 = 2745. (IFCLENGTHMEASURE) [MILLI METRE]
    CONNECTOR0_dZ_01 = 2825. (IFCLENGTHMEASURE) [MILLI METRE]
    CONNECTOR0_ref_dZ = 2745. (IFCLENGTHMEASURE) [MILLI METRE]
    CONNECTOR1_DIAMETER_dZ_0r = 125. (IFCLENGTHMEASURE) [MILLI METRE]
    CONNECTOR1_dZ_01 = 80. (IFCLENGTHMEASURE) [MILLI METRE]
    CONNECTOR1_ref_dZ = 80. (IFCLENGTHMEASURE) [MILLI METRE]
  Graphics | properties | on 1 object (1 IFCFLOWFITTING)
    Use Annotation Scale = FALSE (IFCBOOLEAN)
  Graphics | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Mitte (1)" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "M_Ebenenbeschriftung - Kreis: M_Ebenenbeschriftung - Kreis" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Insulation | properties | on 1 object (1 IFCFLOWFITTING)
    Insulation Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall Size = "125 mmø-125 mmø" (IFCTEXT)
  Mechanical | properties | on 1 object (1 IFCFLOWFITTING)
    Loss Method = "3bf616f9-6b98-4a21-80ff-da1120c8f6d6" (IFCTEXT)
    System Abbreviation = "" (IFCTEXT)
    System Classification = "Undefined" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Phasing | properties | on 1 object (1 IFCFLOWFITTING)
    Phase Created = "Neue Konstruktion" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  Data | properties | on 1 type object
    Außendurchmesser Rohr [mm] = 133. (IFCREAL)
    Index Number = 8. (IFCREAL)
    Lieferlänge [m] = 2.75 (IFCREAL)
    Nutzbare Rohrlänge [m] = 2.75 (IFCREAL)
    Rohrgewicht pro Meter (leer) [kg/m] = 8. (IFCREAL)
    Wanddicke [mm] = 2.5 (IFCREAL)
    Wärmeausdehnungskoeffizient Rohr [mm/(m.K)] = 0.0117 (IFCREAL)
    max. zul. Dauer-Betriebstemperatur [°C] Number = 95. (IFCREAL)
  General | properties | on 1 type object
    BIM = "https://media.stage.bim.site/t/eyJhbGciOiJIUzI1NiIsInR5cCI6IkpXVCJ9.eyJjdCI6MSwidGYiOiJwdWJsaWMvbG9yb3dlcmsta2gtdmFobGJyYXVrLWdtYmgtY28ta2cvZjVhMjlmMS9QQVJUMjlfTG9yb18yMDE5MDcwMV8xLlZESSIsImNpZCI6IjMyNzdjYzIzLTgxYTktNGVlMy1hOTBhLWI0N2JiNGMwYjYxNiIsInJpZCI6ImVhMjdkZDQ4MmIxOWJlNGU3ZmQyNWYwYjAwNGViODM0IiwicGlkIjoiZmExNzFlZjI3NDA2MmZkNjhiNDZmNmZlNWU5MDhlNDgwYjZkM2ZjOCIsInNpZCI6IjY2MzI1IiwidXQiOjUsImxjIjoiZGUiLCJpYXQiOjE1NjcxMzY4NTQsImlzcyI6Imh0dHBzOi8vYXBpLmxpdmUuYmltLnNpdGUiLCJzdWIiOiJyZXZpdC50ZWFtMjRAZ21haWwuY29tIn0.nbTuOF5MWwUuXpqjeCQVM3Iqnh04-OIhscT0qbqN5Zc/PART29_Loro_20190701_1.VDI" (IFCTEXT)
    Brandschutzklasse Text = "B1 nach DIN 4102" (IFCTEXT)
    HeinzeBIM = "https://www.heinze.de/bim/loro-x-rohre-mit-einer-muffe/fa171ef274062fd68b46f6fe5e908e480b6d3fc8" (IFCTEXT)
    Lieferform = "Stück" (IFCTEXT)
    Nenndruck Text = "0.5" (IFCTEXT)
    Nenndrucksystem Text = "PN" (IFCTEXT)
    Nennmaß = "125" (IFCTEXT)
    Nennweitensystem Text = "DN" (IFCTEXT)
    Normen/Regeln/Zulassungen Text = "DVGW für Trinkwasser" (IFCTEXT)
    Produktbezeichnung Text = "LORO-X Stahlabflussrohre" (IFCTEXT)
    Produktkennung Text = "Rohr" (IFCTEXT)
    Produktname Text = "LORO-X Rohre mit einer Muffe" (IFCTEXT)
    Produktvideo = "https://media.stage.bim.site/t/eyJhbGciOiJIUzI1NiIsInR5cCI6IkpXVCJ9.eyJjdCI6MiwidHUiOiJodHRwOi8vd3d3Lmxvcm8uZGUvaW5kZXgucGhwP2lkPTIzM1x1MDAyNmFydGlrZWxucj0wMTAwNS4xMjVYIiwiY2lkIjoiMzI3N2NjMjMtODFhOS00ZWUzLWE5MGEtYjQ3YmI0YzBiNjE2IiwicmlkIjoiZWEyN2RkNDgyYjE5YmU0ZTdmZDI1ZjBiMDA0ZWI4MzQiLCJwaWQiOiJmYTE3MWVmMjc0MDYyZmQ2OGI0NmY2ZmU1ZTkwOGU0ODBiNmQzZmM4Iiwic2lkIjoiNjYzMjUiLCJ1dCI6MiwibGMiOiJkZSIsImlhdCI6MTU2NzEzNjg1NCwiaXNzIjoiaHR0cHM6Ly9hcGkubGl2ZS5iaW0uc2l0ZSIsInN1YiI6InJldml0LnRlYW0yNEBnbWFpbC5jb20ifQ.cSQTVR8T-COpspaol9Q4KcX1IWNAvLhJyjDv5q4C6mo" (IFCTEXT)
    Querschnittsform Text = "rund" (IFCTEXT)
    Verbindungsart I Text = "Pressen" (IFCTEXT)
    Verbindungsart II Text = "axial pressen" (IFCTEXT)
    Verlegeart Text = "Unterputz" (IFCTEXT)