IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "Projektnummer"
Time stamp: "2019-08-22T12:34:51"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20160225_1515(x64) - Exporter 17.0.416.0 - Alternate UI 17.12.14.0"
Application: "Autodesk Revit 2017 (ENU)" version "2017" identifier "Revit" by Organization "Autodesk Revit 2017 (ENU)"

People and organizations
  Person "Peace" of Organization (no name given)
  Owner history of Person "Peace" of Organization (no name given) | application "Autodesk Revit 2017 (ENU)" version "2017" identifier "Revit" by Organization "Autodesk Revit 2017 (ENU)" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "Projektnummer" | long name "Projektname" | phase "Projektstatus"
  IFCSITE "Default" | latitude 42° 12′ 46.804504″ | longitude -71° 2′ 0.602416″ | elevation above sea level 0.
    IFCBUILDING | postal address: "## Straße Ort, Bundesland PLZ", "Boston", "MA"
      IFCBUILDINGSTOREY "Ebene 1" | long name "Ebene 1" | elevation 0.
        contains 1 element
          1 x IFCFLOWTERMINAL | object type "LOROWERK 21516-100X" | names: "LOROWERK 21516-100X:LOROWERK 21516-100X:237126" | material: materials ("ConnectorOutletMediumMaterial", "ConnectorInletMediumMaterial", "Material_12013", "Material_12011", "Material_12010", "Material_12012") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Constraints, Dimensions, Identity Data, Mechanical

Property sets
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
    Client Name = "Besitzer" (IFCTEXT)
    Project Address = "## Straße Ort, Bundesland PLZ" (IFCTEXT)
    Project Issue Date = "Ausgabedatum" (IFCTEXT)
    Project Name = "Projektname" (IFCTEXT)
    Project Number = "Projektnummer" (IFCTEXT)
    Project Status = "Projektstatus" (IFCTEXT)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Other | properties | on 1 object (1 IFCFLOWTERMINAL)
    Category = "Plumbing Fixtures" (IFCLABEL)
    Family = "LOROWERK 21516-100X: LOROWERK 21516-100X" (IFCLABEL)
    Family and Type = "LOROWERK 21516-100X: LOROWERK 21516-100X" (IFCLABEL)
    Type = "LOROWERK 21516-100X: LOROWERK 21516-100X" (IFCLABEL)
    Type Id = "LOROWERK 21516-100X: LOROWERK 21516-100X" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: 8 mm Kopf" (IFCLABEL)
    Family and Type = "Level: 8 mm Kopf" (IFCLABEL)
    Type = "Level: 8 mm Kopf" (IFCLABEL)
    Type Id = "Level: 8 mm Kopf" (IFCLABEL)
  Other | properties | on 1 object (1 IFCFLOWTERMINAL)
    Category = "Plumbing Fixtures" (IFCLABEL)
    Family Name = "LOROWERK 21516-100X" (IFCTEXT)
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "8 mm Kopf" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCFLOWTERMINAL)
    Mark = "40" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Ebene 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 object (1 IFCFLOWTERMINAL)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    DATANORM = "21516.100X" (IFCTEXT)
    Description = "LORO-DRAINLET DL Flachdachabläufe, Kompletteinheiten, einteilig" (IFCTEXT)
    GTIN = "4038088085868" (IFCTEXT)
    HAN = "21516.100X" (IFCTEXT)
    Manufacturer = "LOROWERK K.H. Vahlbrauk GmbH & Co. KG" (IFCTEXT)
    OmniClass Number = "" (IFCTEXT)
    OmniClass Title = "" (IFCTEXT)
    Type Name = "LOROWERK 21516-100X" (IFCTEXT)
    VDIBSN = "0020030000020010000010010020010000000030020000002000000001" (IFCTEXT)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCFLOWTERMINAL)
    Manufacturer = "LOROWERK K.H. Vahlbrauk GmbH & Co. KG" (IFCLABEL)
  Pset_DistributionFlowElementCommon | properties | on 1 object (1 IFCFLOWTERMINAL)
    Reference = "LOROWERK 21516-100X" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCFLOWTERMINAL)
    Host = "Level : Ebene 1" (IFCTEXT)
    Level = "Level: Ebene 1" (IFCLABEL)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Dimensions | properties | on 1 object (1 IFCFLOWTERMINAL)
    Area = 0.400333029893907 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.040048195259251 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCFLOWTERMINAL)
    CONNECTOR0_DIAMETER_dZ_0r = 100. (IFCLENGTHMEASURE) [MILLI METRE]
    CONNECTOR0_dZ_00 = 12. (IFCLENGTHMEASURE) [MILLI METRE]
    CONNECTOR0_dZ_01 = 12.79375 (IFCLENGTHMEASURE) [MILLI METRE]
    CONNECTOR0_ref_dZ = 12.79375 (IFCLENGTHMEASURE) [MILLI METRE]
    CONNECTOR1_DIAMETER_dNBN0_0r = 100. (IFCLENGTHMEASURE) [MILLI METRE]
    CONNECTOR1_dNBN0_00 = 39.9532724922226 (IFCLENGTHMEASURE) [MILLI METRE]
    CONNECTOR1_dNBN0_01 = 289.953272492223 (IFCLENGTHMEASURE) [MILLI METRE]
    CONNECTOR1_ref_dNBN0 = 39.9532724922226 (IFCLENGTHMEASURE) [MILLI METRE]
    CONNECTOR1_ref_dNBN1 = 86.8807787918216 (IFCLENGTHMEASURE) [MILLI METRE]
  Mechanical | properties | on 1 object (1 IFCFLOWTERMINAL)
    System Abbreviation = "" (IFCTEXT)
    System Classification = "Undefined" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Phasing | properties | on 1 object (1 IFCFLOWTERMINAL)
    Phase Created = "Neue Konstruktion" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  Data | properties | on 1 object (1 IFCFLOWTERMINAL)
    38.710.01.13 = "seitlich" (IFCTEXT)
    38.710.01.5 = "DN" (IFCTEXT)
    Bestellmenge (Multiplikator) Number = 1. (IFCREAL)
  General | properties | on 1 object (1 IFCFLOWTERMINAL)
    Abdichtvarianten = "mit Klemmflansch" (IFCTEXT)
    Abflussstutzen Ausführung = "waagerecht" (IFCTEXT)
    Ablaufanschluss = "1" (IFCTEXT)
    Art der Nenn-/ Betriebsspannung = "nicht zutreffend" (IFCTEXT)
    BIM = "https://media.stage.bim.site/t/eyJhbGciOiJIUzI1NiIsInR5cCI6IkpXVCJ9.eyJjdCI6MSwidGYiOiJwdWJsaWMvbG9yb3dlcmsta2gtdmFobGJyYXVrLWdtYmgtY28ta2cvZDMwZTRjMS9QQVJUMzhfTG9yb18yMDE5MDcwMV8xLlZESSIsImNpZCI6IjMyNzdjYzIzLTgxYTktNGVlMy1hOTBhLWI0N2JiNGMwYjYxNiIsInJpZCI6IjA1NjQ0MDMxYmM4ZTQyY2MxZjY1M2Y3MzVkYzM0ZmRkIiwicGlkIjoiZWI2NTZjYjJkNTkwNjMzYTEyNWY2MWIzMThjMjhhM2NhNDM1Yzk4NyIsInNpZCI6IjY2MzI1IiwidXQiOjUsImxjIjoiZGUiLCJpYXQiOjE1NjU4NDczNzAsImlzcyI6Imh0dHBzOi8vYXBpLmxpdmUuYmltLnNpdGUiLCJzdWIiOiJyZXZpdC50ZWFtMjRAZ21haWwuY29tIn0.G-wIOMXzAouBZNhxGKycdRGXs5GeM8iRlXM5fRm83WI/PART38_Loro_20190701_1.VDI" (IFCTEXT)
    Elektrischer Anschluss = "nein" (IFCTEXT)
    Feuerwiderstandsklasse = "keine Feuerwiderstandsklasse" (IFCTEXT)
    Feuerwiderstandsklasse nachrüstbar = "nein" (IFCTEXT)
    Gehäuseanschlussarten = "Ablauf punktförmig" (IFCTEXT)
    Geruchsverschluss = "ohne Geruchsverschluss" (IFCTEXT)
    HeinzeBIM = "https://www.heinze.de/bim/loro-dl-ablauf-edelstahl-klemmflansch-seitl-1-tlg-wd-u-heizung-dn100/eb656cb2d590633a125f61b318c28a3ca435c987" (IFCTEXT)
    Heizung = "mit Heizung" (IFCTEXT)
    Kommentar = "Kompletteinheit Serie 84 einteilig" (IFCTEXT)
    Nenndruck Text = "438" (IFCTEXT)
    Nenndrucksystem Text = "300" (IFCTEXT)
    Nennweitensystem Text = "PN" (IFCTEXT)
    Potenzialausgleich (Erdungsanschluss) vorhanden = "ja" (IFCTEXT)
    Produktbezeichnung Text = "LORO-DL Ablauf, Edelstahl, Klemmflansch, seitl., 1-tlg., WD u. Heizung, DN100" (IFCTEXT)
    Produktklassifikation = "Flachdachablauf" (IFCTEXT)
    Produktname Text = "LORO-DL Ablauf, Edelstahl, Klemmflansch, seitl., 1-tlg., WD u. Heizung, DN100" (IFCTEXT)
    Produktvideo = "https://media.stage.bim.site/t/eyJhbGciOiJIUzI1NiIsInR5cCI6IkpXVCJ9.eyJjdCI6MiwidHUiOiJodHRwOi8vd3d3Lmxvcm8uZGUvaW5kZXgucGhwP2lkPTIzM1x1MDAyNmFydGlrZWxucj0yMTUxNi4xMDBYIiwiY2lkIjoiMzI3N2NjMjMtODFhOS00ZWUzLWE5MGEtYjQ3YmI0YzBiNjE2IiwicmlkIjoiMDU2NDQwMzFiYzhlNDJjYzFmNjUzZjczNWRjMzRmZGQiLCJwaWQiOiJlYjY1NmNiMmQ1OTA2MzNhMTI1ZjYxYjMxOGMyOGEzY2E0MzVjOTg3Iiwic2lkIjoiNjYzMjUiLCJ1dCI6MiwibGMiOiJkZSIsImlhdCI6MTU2NTg0NzM3MCwiaXNzIjoiaHR0cHM6Ly9hcGkubGl2ZS5iaW0uc2l0ZSIsInN1YiI6InJldml0LnRlYW0yNEBnbWFpbC5jb20ifQ.g1GF2IfQHVbjVH15BSW34rBoJAeLDBi4dVLjiUtNQ80" (IFCTEXT)
    Typ = "Dachablauf" (IFCTEXT)
    Werkstoff des Ablaufkörpers = "nicht rostender Stahl" (IFCTEXT)
    Wärmedämmung = "mit Wärmedämmung" (IFCTEXT)
  Graphics | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Mitte (1)" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "M_Ebenenbeschriftung - Kreis: M_Ebenenbeschriftung - Kreis" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)