IFC building model
Schema: "IFC4"
Description: "ViewDefinition [ReferenceView_V1.0]"
File name: "Projektnummer"
Time stamp: "2019-09-08T12:24:24"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20160225_1515(x64) - Exporter 17.0.416.0 - Alternate UI 17.12.14.0"
Application: "Autodesk Revit 2017 (DEU)" version "2017" identifier "Revit" by Organization "Autodesk Revit 2017 (DEU)"

People and organizations
  Person "AMAR" of Organization (no name given)
  Owner history of Person "AMAR" of Organization (no name given) | application "Autodesk Revit 2017 (DEU)" version "2017" identifier "Revit" by Organization "Autodesk Revit 2017 (DEU)" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "Projektnummer" | long name "Projektname" | phase "Projektstatus"
  IFCSITE "Default" | latitude 42° 12′ 46.804504″ | longitude -71° 2′ 0.602416″ | elevation above sea level 0.
    IFCBUILDING | postal address: "## Straße Ort, Bundesland PLZ", "Boston", "MA"
      IFCBUILDINGSTOREY "Ebene 1" | long name "Ebene 1" | elevation 0.
        contains 1 element
          1 x IFCBUILDINGELEMENTPROXY | object type "LOROWERK 01372.050X" | USERDEFINED | names: "LOROWERK 01372.050X:LOROWERK 01372.050X:301473" | material: materials ("ConnectorOutletMediumMaterial", "ConnectorInletMediumMaterial", "Material_17179") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Abhängigkeiten, Abmessungen, HLS, ID-Daten

Property sets
  Sonstige | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Kategorie = "Projektinformationen" (IFCLABEL)
    Kundenname = "Besitzer" (IFCTEXT)
    Projektadresse = "## Straße Ort, Bundesland PLZ" (IFCTEXT)
    Projektausgabedatum = "Ausgabedatum" (IFCTEXT)
    Projektname = "Projektname" (IFCTEXT)
    Projektnummer = "Projektnummer" (IFCTEXT)
    Projektstatus = "Projektstatus" (IFCTEXT)
  Sonstige | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Familienname = "Ebene" (IFCTEXT)
    Kategorie = "Ebenen" (IFCLABEL)
  Sonstige | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Familie = "LOROWERK 01372.050X: LOROWERK 01372.050X" (IFCLABEL)
    Familie und Typ = "LOROWERK 01372.050X: LOROWERK 01372.050X" (IFCLABEL)
    Kategorie = "Sanitärinstallationen" (IFCLABEL)
    Typ = "LOROWERK 01372.050X: LOROWERK 01372.050X" (IFCLABEL)
    Typ-ID = "LOROWERK 01372.050X: LOROWERK 01372.050X" (IFCLABEL)
  Sonstige | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Familie = "Ebene: 8 mm Kopf" (IFCLABEL)
    Familie und Typ = "Ebene: 8 mm Kopf" (IFCLABEL)
    Kategorie = "Ebenen" (IFCLABEL)
    Typ = "Ebene: 8 mm Kopf" (IFCLABEL)
    Typ-ID = "Ebene: 8 mm Kopf" (IFCLABEL)
  Sonstige | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Familienname = "LOROWERK 01372.050X" (IFCTEXT)
    Kategorie = "Sanitärinstallationen" (IFCLABEL)
  ID-Daten | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Autor = "" (IFCTEXT)
    Beschreibung von Unternehmen = "" (IFCTEXT)
    Gebäudename = "" (IFCTEXT)
    Unternehmensname = "" (IFCTEXT)
  ID-Daten | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Typname = "8 mm Kopf" (IFCTEXT)
  ID-Daten | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Kennzeichen = "4" (IFCTEXT)
  ID-Daten | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Gebäudegeschoss = TRUE (IFCBOOLEAN)
    Name = "Ebene 1" (IFCTEXT)
    Tragwerk = FALSE (IFCBOOLEAN)
  ID-Daten | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Baugruppenbeschreibung = "" (IFCTEXT)
    Baugruppenkennzeichen = "" (IFCTEXT)
    Beschreibung = "LORO-RAINSTAR Attikaabläufe, Serie 79" (IFCTEXT)
    Codename = "" (IFCTEXT)
    DATANORM = "01372.050X" (IFCTEXT)
    GTIN = "4038088072875" (IFCTEXT)
    HAN = "01372.050X" (IFCTEXT)
    Hersteller = "LOROWERK K.H. Vahlbrauk GmbH & Co. KG" (IFCTEXT)
    OmniClass-Nummer = "" (IFCTEXT)
    OmniClass-Titel = "" (IFCTEXT)
    Typname = "LORO-RAINSTAR 79 Attikaablauf, Edelst., Klemmfl., f. Kunstst.-bahn, Freispiegel, DN50" (IFCTEXT)
    VDIBSN = "0020050000020010000010020010010000000030020000000400000001" (IFCTEXT)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    FireRating = "keine Feuerwiderstandsklasse" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "LOROWERK 01372.050X" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Manufacturer = "LOROWERK K.H. Vahlbrauk GmbH & Co. KG" (IFCLABEL)
  Abhängigkeiten | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Basisbauteil = "Ebene : Ebene 1" (IFCTEXT)
    Ebene = "Ebene: Ebene 1" (IFCLABEL)
    Versatz = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Abhängigkeiten | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Ansicht = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Abhängigkeiten | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Basishöhe = "Projekt-Basispunkt" (IFCIDENTIFIER)
  Abmessungen | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Fläche = 0.557552300521175 (IFCAREAMEASURE) [SQUARE_METRE]
    Volumen = 0.0604795362674352 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Abmessungen | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Höhe für Berechnung = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Abmessungen | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    CONNECTOR0_DIAMETER_dZ_0r = 125. (IFCLENGTHMEASURE) [MILLI METRE]
    CONNECTOR0_dZ_00 = 17.5 (IFCLENGTHMEASURE) [MILLI METRE]
    CONNECTOR0_dZ_01 = 18.29375 (IFCLENGTHMEASURE) [MILLI METRE]
    CONNECTOR0_ref_dZ = 18.29375 (IFCLENGTHMEASURE) [MILLI METRE]
    CONNECTOR1_DIAMETER_dNBN0_0r = 50. (IFCLENGTHMEASURE) [MILLI METRE]
    CONNECTOR1_dNBN0_00 = 757.679382555729 (IFCLENGTHMEASURE) [MILLI METRE]
    CONNECTOR1_dNBN0_01 = 798.679382555729 (IFCLENGTHMEASURE) [MILLI METRE]
    CONNECTOR1_ref_dNBN0 = 757.679382555729 (IFCLENGTHMEASURE) [MILLI METRE]
    CONNECTOR1_ref_dNBN1 = 49.604719945663 (IFCLENGTHMEASURE) [MILLI METRE]
  HLS | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Systemabkürzung = "" (IFCTEXT)
    Systemklassifizierung = "Nicht definiert" (IFCTEXT)
    Systemname = "" (IFCTEXT)
  Phasen | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Phase erstellt = "Neue Konstruktion" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
    Reference = "Projektinformationen" (IFCIDENTIFIER)
  Allgemein | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Abdichtvarianten = "mit Klemmflansch" (IFCTEXT)
    Abflussstutzen Ausführung = "waagerecht" (IFCTEXT)
    Ablaufanschluss = "1" (IFCTEXT)
    Art der Nenn-/Betriebsspannung = "nicht zutreffend" (IFCTEXT)
    BIM = "https://media.stage.bim.site/t/eyJhbGciOiJIUzI1NiIsInR5cCI6IkpXVCJ9.eyJjdCI6MSwidGYiOiJwdWJsaWMvbG9yb3dlcmsta2gtdmFobGJyYXVrLWdtYmgtY28ta2cvZDMwZTRjMS9QQVJUMzhfTG9yb18yMDE5MDcwMV8xLlZESSIsImNpZCI6IjMyNzdjYzIzLTgxYTktNGVlMy1hOTBhLWI0N2JiNGMwYjYxNiIsInJpZCI6ImNkZmZlNzU3ZWFjYTE3ZTNlZGU0M2Q0ZjhkZjA3NWEzIiwicGlkIjoiZWZmMjY2NzQyMWQzY2Y3YWMyNDA2ZTJmOWExOTY2Y2U0M2ViZjZiOSIsInNpZCI6IjY2MzI1IiwidXQiOjUsImlhdCI6MTU2NTA5MTg1MywiaXNzIjoiaHR0cHM6Ly9hcGkubGl2ZS5iaW0uc2l0ZSIsInN1YiI6ImFkbWluQGJpbXNpdGUuZGV2In0.gyy-AbC1IlYbkiA80gKlqHfgIx_1QEWkF-Lsy8z9Xls/PART38_Loro_20190701_1.VDI" (IFCTEXT)
    Feuerwiderstandsklasse = "keine Feuerwiderstandsklasse" (IFCTEXT)
    Feuerwiderstandsklasse nachrüstbar = "nein" (IFCTEXT)
    Gehäuseanschlussarten = "Ablauf punktförmig" (IFCTEXT)
    Geruchsverschluss = "ohne Geruchsverschluss" (IFCTEXT)
    Heizung = "ohne Heizung" (IFCTEXT)
    Ist System = FALSE (IFCBOOLEAN)
    Ist Zubehör = FALSE (IFCBOOLEAN)
    Kommentar = "Serie 79" (IFCTEXT)
    Nenndruck = "936" (IFCTEXT)
    Nenndrucksystem = "270" (IFCTEXT)
    Nennweitensystem = "PN" (IFCTEXT)
    Potenzialausgleich (Erdungsanschluss) vorhanden = "ja" (IFCTEXT)
    Produktbezeichnung = "LORO-RAINSTAR 79 Attikaablauf, Edelst., Klemmfl., f. Kunstst.-bahn, Freispiegel, DN50" (IFCTEXT)
    Produktklassifikation = "Attikaablauf" (IFCTEXT)
    Produktname = "LORO-RAINSTAR 79 Attikaablauf, Edelst., Klemmfl., f. Kunstst.-bahn, Freispiegel, DN50" (IFCTEXT)
    Produktvideo = "https://media.stage.bim.site/t/eyJhbGciOiJIUzI1NiIsInR5cCI6IkpXVCJ9.eyJjdCI6MiwidHUiOiJodHRwOi8vd3d3Lmxvcm8uZGUvaW5kZXgucGhwP2lkPTIzM1x1MDAyNmFydGlrZWxucj0wMTM3Mi4wNTBYIiwiY2lkIjoiMzI3N2NjMjMtODFhOS00ZWUzLWE5MGEtYjQ3YmI0YzBiNjE2IiwicmlkIjoiY2RmZmU3NTdlYWNhMTdlM2VkZTQzZDRmOGRmMDc1YTMiLCJwaWQiOiJlZmYyNjY3NDIxZDNjZjdhYzI0MDZlMmY5YTE5NjZjZTQzZWJmNmI5Iiwic2lkIjoiNjYzMjUiLCJ1dCI6MiwiaWF0IjoxNTY1MDkxODUzLCJpc3MiOiJodHRwczovL2FwaS5saXZlLmJpbS5zaXRlIiwic3ViIjoiYWRtaW5AYmltc2l0ZS5kZXYifQ.EFX4nZu1s5FPg0rNtGEBvP44UjZnI8gp1_sQM4zjIqo" (IFCTEXT)
    Werkstoff des Ablaufkörpers = "nicht rostender Stahl" (IFCTEXT)
    Wärmedämmung = "ohne Wärmedämmung" (IFCTEXT)
    elektrischer Anschluss = "nein" (IFCTEXT)
  Daten | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    38.710.01.13 = "seitlich" (IFCTEXT)
    38.710.01.5 = "DN" (IFCTEXT)
    Bestellmenge (Multiplikator) = 1. (IFCREAL)
    Einbaubreite [m] = 0.239 (IFCREAL)
    Einbautiefe [m] = 0. (IFCREAL)
    Sperrwasserhöhe [m] = 0. (IFCREAL)
  Grafiken | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Farbe = 0 (IFCINTEGER)
    Linienmuster = "Mitte (1)" (IFCLABEL)
    Linienstärke = "1" (IFCIDENTIFIER)
    Symbol = "M_Ebenenbeschriftung - Kreis: M_Ebenenbeschriftung - Kreis" (IFCLABEL)
    Symbol bei Ende 1 Standard = FALSE (IFCBOOLEAN)
    Symbol bei Ende 2 Standard = TRUE (IFCBOOLEAN)